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September 29th, 2025
Decora Homes / RRD Construction Group
826 47th Street East 	Saskatoon, SK





Ready-to-Move Home Build Proposal - The Hawk	
James Smith Cree Nation  


OVERVIEW

· PROPERTY LOCATION: 		James Smith Cree Nation, SK  
· MAIN FLOOR:		1094 square feet 
· BASEMENT:		1094 square feet
· This sheet outlines the specifications and inclusions of a completed Ready-to-Move home build and does not include or imply alternate or extra budget amounts or associated costs not listed
· The proposed specification sheet is based on “The Hawk” preliminary concept floor plans and exterior renderings of a 1094 square foot ready-to-move bungalow home with an ICF foundation and finished basement 
· Homes to be yard built in Saskatoon and transported to James Smith Cree Nation 
· Foundation and finished basement completed on James Smith Cree Nation
· Engineering stamp is provided by Decora Homes / RRD Construction Group if required
· Blueprints are provided by Decora Homes / RRD Construction Group
· Final drawings to be finalized and signed between builder and client for approval 
· New Home Warranty by Progressive Warranty supplied through Decora Homes / RRD Construction Group


BUILDING STRUCTURE SPECIFICATIONS
· Foundation				
· This spec sheet includes the following structure built on site:
· Concrete strip footings: 20MPA Type HS concrete  with reinforcing
· Telepost pads: 20MPA Type HS concrete with reinforcing
· Foundation walls: 8” x 8’-0” insulated concrete forms with 25MPA Type HS reinforced concrete
· Basement Floor: 20MPA Type HS 3” depth poured 6 MIL poly ground cover and 6” granular fill  
· Waterproofing applied to exterior foundation walls below grade
· Weeping tile installed around perimeter of house foundation walls covered by 6” of crushed rock and drained into sump system as required 



· Framing 
· Framing package includes but is not limited to:
· Main Floor System: Engineered I-joists supplied by manufacturer
· Exterior Walls: 2x6 SPF studs spaced at 24” on center
· Exterior Sheathing: 3/8” OSB 
· Interior Walls: 2x4 & 2x6 SPF studs spaced at 16” unless noted otherwise
· Interior Sheathing: ½” plywood sheathing 
· Subfloor: ¾” T&G OSB screwed and glued
· Roof Trusses: Engineered truss system designed by manufacturer
· Roof Sheathing: 7/16” OSB



· Roofing
· Standard IKO Cambridge Architectural Shingles
· Metal Roof & Drip Edge and Flashings
· Ice and Water Shield
· Underlayment as required
· Roof Vents as required



· Ceiling Heights
· Main Floor:		8 feet  
· Basement:		7.75 feet 





· Thermal Insulation
· Main Floor and Basement Insulation includes:
· Exterior Walls:	R20 Fiberglass batt insulation
· Basement Walls: R23 Insulated Concrete Forms 
· Ceiling: R40 Fiberglass blown-in or batt insulation
· Windows & Doors: Hilti Spray-Applied insulation

· All exterior walls and ceilings to be sealed with 6mm CGSB polyethylene vapor barrier


· Exterior Windows & Doors
· Windows:
· Energy Star rating 
· Exterior finish color - White 
· Interior fInish color - White 
· Fixed, awning & sliding windows 
· Screens included on operable windows 
· Exterior Door(s)
· 1/4 Lite Front Door 
· Full Lite Covered Deck Door 
· Patio or Garden Door to Rear Yard 
· Door Finish 
· Paint grade finish interior and exterior 

	

· Exterior Finish
· Exterior Siding: 		
· Vinyl Siding
· Profiles and Colours TBD
· Weather Barrier
· Flashings, Fasteners, Trims & Accessories

· Soffit, Fascia & Eaves: 			
· Soffit & Fascia 
· 6” Prefinished Fascia Board 
· Vented and non-vented soffit as required 
· Eavestrough & Downspouts
· Eavestrough with standard downspouts
· Matched to soffit and fascia color


· Exterior Front Stair 
· Pressure treated wood framed landing and steps with railing  

· Covered Deck
· Pressure treated wood framed deck with railing as required 


· Driveway 
· Not Included 


· Landscaping 
· Not Included 





ELECTRICAL SPECIFICATIONS
· Electrical Overview
· Electrical fixture package included
· Flush mount 3000K LED round ceiling fixtures 
· Electrician Overview
· Any work done by the electrician in the house will be part of this scope.  Some items that will/can be covered include but are not limited to:
· House electrical panel will be wired into provided SaskPower electrical service 
· Low voltage switching installed for ventilation system
· Carbon monoxide and smoke detectors wired
· Any light junction boxes and installation of any light fixtures
· Wiring of appliances






MECHANICAL & PLUMBING SPECIFICATIONS
· Forced Air Heating & Cooling
· Natural Gas Energy Star Furnace 
· Sized by mechanical contractor 
· Equipment warranty as per manufacturer
· White plastic supply registers
· White metal return air grills 
· HRV unit with main control and timers 
· Main gas line is included with the heating system. 
· Including gas line from gas meter on house to basement and lines to all supplied gas-fired equipment
· SaskEnergy service and line on site up to the house including the meter is the responsibility of the reservation 
· Plumbing 
· 4" sewer main line from inside footing
· Sewer hookup & piping on site up to the house footing is the responsibility of the reservation
· Standard water system with 3/4" main line and 1/2" branch lines to fixtures
· Water hookup, meter & piping on site up to the house is the responsibility of the reservation
· ABS drainage and ventilation
· Water heater
· Sump pump and pit drain to rear of house if required 
· Radon trap supply
· Fixture Setting throughout
· Dishwasher hookup 
· Laundry hookup 


· Plumbing Fixtures
· Plumbing fixtures, trims and valves
· Includes matching towel rod, towel ring and toilet paper holder



INTERIOR FINISH SPECIFICATIONS

· Wall & Ceiling Finish
· Walls to be durable finish 
· Includes ½” plywood underneath finish
· Ceilings to be 1⁄2” drywall
· Ceilings will have knockdown textured finish 
· Basement foundation interior wall to be durable wall finish over 
· Includes ½” plywood underneath finish 
· Any other wall or ceiling finishes are not included


· Painting
· Walls to have painted finish
· Trim work and interior doors are finish with a latex paint in a white finish
· MDF closets which are painted to match the wall paint in their respective rooms
· One colour included throughout home


· Flooring Finish
· Main Floor Flooring - Click luxury vinyl plank
· Basement Flooring - Glue down luxury vinyl plank

· Finish Carpentry
· Finish Carpentry Labour
· Installation of interior doors, door & window casing, baseboards, closet rods and washroom accessories 

· Interior Finish Material Package Supply
· Items that will be covered include, but are not limited to: 
· 6’8” hollow core doors 
· MDF Baseboard & MDF casing
· MDF for standard closet shelves 
· Door knobs
· Hinges, stops, roller catches and deadbolt 
· Closet rods 


· Cabinets & Countertops
· Cabinetry package includes kitchen millwork and bathroom vanity 
· Includes standard handles
· Arborite countertops throughout


· Appliances
· Base appliance package included:
· Stainless Steel: kitchen range,over-the-range microwave,
dishwasher, refrigerator
· White stacked laundry unit   


· Glass & Mirrors
· Standard mirror included at bathroom sink 
· Shower glass is not included 



· Window Coverings
· Not Included 



· Furniture
· Not Included


MISCELLANEOUS
· Overview
· Progressive Home Warranty Certificate Provided
· Permits and fees which are incurred during construction are included
· Home moving from Saskatoon yard to onsite foundation included 
· Insurance coverage during construction and transportation is included
· Surveyor's Certificate Provided
· Home cleaned before possession 




All changes made to plans including change orders need to be approved by the builder and client in writing.  
Any change orders must be paid for up-front before work commences.
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